# Controller Window

The controller window is your central control center of your device. You can access and control the DSP functionality (EQ, level, delay, etc.), input and output routing and device system information and options.

Mission Control - Controller Window

(1) Device Name(1) Device Name

The name of your device is displayed here. You can change the name by simply click on the field and enter your new desired name. After pressing enter, the new name is synchronized with your real device.

(2) Device Preset(2) Device Preset

This field shows the current preset that is active on this device. The field provides also access to the list of available device presets. Click on the small down-facing arrow and select a preset. After you have made your choice, a pop-window is shown with the request for your confirmation to load and activate the selected preset.

(3) Preset Options(3) Preset Options

The preset options menu lets you manage, save, overwrite, revert, export and import presets.

(4) System Status(4) System Status

The system status pane provides an overview of the entire system. You can monitor temperature, network and sync status and get information about firmware version, device serial number and input state.

(5) Dashboard(5) Dashboard

In the dashboard tab all channels of your device are displayed with the main information. You can quickly access channel gain, output routing, mute, phase and also see level and signal input information.

(6) Channel(6) Channel

A separate tab is available for each channel of the unit, allowing detailed control of the functions and signal processing of the respective channel.

(7) Channel Gain(7) Channel Gain

Control channel input gain with the fader or entry field.

(8) Output Level Indicator(8) Output Level Indicator

Displays the level of the output in real-time.

(9) RMS Limiter Charging(9) RMS Limiter Charging

Shows the charging of the RMS limiter. Once the charging gets near 100% the limiter starts to reduce the output level.

(10) Gain Reduction Indicator(10) Gain Reduction Indicator

Displays the gain reduction introduced by an active limiter.

(11) Mute and Phase Switch(11) Mute and Phase Switch

Mute or unmute the channel and apply a phase inversion. The buttons indicates their state with different colors.

(12) Signal Indicator(12) Signal Indicator

This LED type indicator blinks when a signal is present. An active mute is indicated by the word "muted". If no signal is present, the indicator shows "No sound".

(13) Channel Output(13) Channel Output

The set channel output is shown here. By clicking on the output indicator the output matrix will open. There you can change the output for this channel.

(14) Add Channel(14) Add Channel

You can add an additional channel by clicking on "Add channel". After you have clicked on "Add channel", a new window will open to set up your new channel. You will be guided through the necessary steps by the system wizard.

(15) Load From File(15) Load From File

With "Load from file" you can load a previously exported channel configuration.