# Channel Controller

The channel control tab shows a single channel. You have access to all DSP and channel features like EQ, delay, gain, input and output routing, etc. The channel tab also provides comprehensive channel relevant information and metering.

Mission Control - Channel Controller

(1) Channel Name and Color(1) Channel Name and Color

The current channel name is displayed here. You can change the naming by entering a new name in the field. Clicking on "Color" enables you to pick a new color for visual channel identification.

(2) Input Meter(2) Input Meter

This meter indicates the input level for the selected input.

(3) Channel Gain(3) Channel Gain

Set channel gain with the fader or entry field.

(4) Output Level Indicator(4) Output Level Indicator

Shows the level of the channel output.

(5) RMS Limiter Charging(5) RMS Limiter Charging

Shows the charging of the RMS limiter. Once the charging gets near 100% the limiter starts to reduce the output level.

(6) Gain Reduction Indicator(6) Gain Reduction Indicator

Displays the gain reduction introduced by an active limiter.

(7) Mute(7) Mute

Mute the output of the channel. Mute state is indicated by different colors.

(8) EQ(8) EQ

Channel Equalizer area with graphical display of set eq parameters.

(9) Channel Delay(9) Channel Delay

Set channel delay in different units. Generally activate or deactivate channel delay.

(10) Polarity Switch (Phase)(10) Polarity Switch (Phase)

Invert polarity of this channel.

(11) Speaker Preset(11) Speaker Preset

The current active channel preset is indicated here. By clicking on the preset name, a new window appears with the option to change the preset. The system wizard will guide you through the necessary steps.

(12) Input Indicator(12) Input Indicator

The selected channel input is indicated. You can click on the channel input name to open the input mix matrix configuration window. You can also set the general input sensitivity here.

(13) Output Indicator(13) Output Indicator

The current output for this physical channel is shown here. By clicking on the indicator the output matrix configuration window will open.

(14) Channel Settings Option(14) Channel Settings Option

You have access to various channel settings. You can copy, save, paste and load settings. You can also delete this physical channel from within this menu.

(15) Add Channel(15) Add Channel

You can add a new channel to your device.

(16) Load From File(16) Load From File

You can load previously exported and saved channels.